{"text_format":"1","workbook":"xlsx","n_sheets":4,"sheets":["opticalCON ADVANCED","opticalCON DRAGONFLY","opticalCON hybrid MED","FIBERFOX"],"not_rendered":{"charts":0,"images":21,"macros":1,"external_links":0,"defined_names":12,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"opticalCON ADVANCED","index":0,"n_rows":43,"n_cols":6,"rows_kept":43,"cut":false,"hidden":false,"merged":[[3,0,3,5],[42,0,46,5]]}
[]
[]
[]
["opticalCON® Advanced Insertion Loss Calculator"]
[]
[]
["1. Mode and wavelength:"]
[]
[]
[]
[]
["2. Connector type:"]
[]
[]
[]
[]
[]
[]
["3. Attenuation properties:"]
[]
["Overal cable length 1)",0,"[m] (e.g. 150m)"]
["Number of connections 2)",0]
["Number of splices 3)",0]
[]
["4. Calculation:"]
[]
[null,null,null,"Typ.","Max."]
["     - Overal cable attenuation",{"$f":"B21/1000","v":0},"km of cable    x",0,0,"dB/km"]
["     - Overal connector attenuation",{"$f":"B22","v":0},"connections    ",0,0,"dB/con. "]
["     - Overal splice attenuation",{"$f":"B23","v":0},"splices            ",0,0,"dB/spl."]
[" = Typical Link attenuation calculated",{"$f":"B28*D28+B29*D29+B30*D30","v":0},"[dB]"]
[" = Maximal Link attenuation calculated",{"$f":"B28*E28+B29*E29+B30*E30","v":0},"[dB]"]
[]
[]
["Notes:"]
["1) ... Summarize the length of all involved cables between transmitter and receiver."]
["2) ... Count the numbers of physical contact connections. The connection into transmitter and receiver has no effect."]
["        Example: Count 4 connections for an installation of two OpticalCon® drums, one OpticalCon® coupler "]
["                       and two patch cables from / to the  transmitting / receiving device."]
["3) ... Running an installation (e.g. into a building) may add several fiber optic splices to a link."]
["        Calculation is based on electrical arc splice technology. ( 0.2dB for Multimode , 0.1dB for Singlemode)"]
[]
["IMPORTANT !\nThis insertion loss calculator works with Excel macros, please select the macro security level \"medium\" or \"low\" when you want to work with it. Choose TOOLS / MACRO / SECURITY in the Excel pulldown menue to select the security level."]

{"sheet":"opticalCON DRAGONFLY","index":1,"n_rows":35,"n_cols":6,"rows_kept":35,"cut":false,"hidden":false,"merged":[[3,0,3,5],[34,0,38,5]]}
[]
[]
[]
["opticalCON® DRAGONFLY Insertion Loss Calculator"]
[]
[]
["1. Mode and wavelength:"]
[]
[]
[]
[]
[]
["2. Attenuation properties:"]
[]
["Overal cable length 1)",0,"[m] (e.g. 150m)"]
["Number of connections 2)",0]
[]
["3. Calculation:"]
[]
[null,null,null,"Typ.","Max."]
["     - Overal cable attenuation",{"$f":"B15/1000","v":0},"km of cable    x",-0.3,-0.3,"dB/km"]
["     - Overal connector attenuation",{"$f":"B16","v":0},"connections    ",-0.6,-1,"dB/con. "]
[" = Typical Link attenuation calculated",{"$f":"B21*D21+B22*D22","v":0},"[dB]"]
[" = Maximal Link attenuation calculated",{"$f":"B21*E21+B22*E22","v":0},"[dB]"]
[]
[]
["Notes:"]
["1) ... Summarize the length of all involved cables between transmitter and receiver."]
["2) ... Count the numbers of expanded beam connections. The LC connection into transmitter and receiver has no effect."]
["        Example: Count 2 connections for one DRAGONFLY cable with two DRAGONFLY chassis. "]
[]
[]
[]
[]
["IMPORTANT !\nThis insertion loss calculator works with Excel macros, please select the macro security level \"medium\" or \"low\" when you want to work with it. Choose TOOLS / MACRO / SECURITY in the Excel pulldown menue to select the security level."]

{"sheet":"opticalCON hybrid MED","index":2,"n_rows":35,"n_cols":6,"rows_kept":35,"cut":false,"hidden":false,"merged":[[3,0,3,5],[34,0,38,5]]}
[]
[]
[]
["opticalCON® hybrid MED Insertion Loss Calculator"]
[]
[]
["1. Mode and wavelength:"]
[]
[]
[]
[]
[]
["2. Attenuation properties:"]
[]
["Overal cable length 1)",0,"[m] (e.g. 150m)"]
["Number of connections 2)",0]
[]
["3. Calculation:"]
[]
[null,null,null,"Typ.","Max."]
["     - Overal cable attenuation",{"$f":"B15/1000","v":0},"km of cable    x",-3,-3,"dB/km"]
["     - Overal connector attenuation",{"$f":"B16","v":0},"connections    ",-0.65,-0.9,"dB/con. "]
[" = Typical Link attenuation calculated",{"$f":"B21*D21+B22*D22","v":0},"[dB]"]
[" = Maximal Link attenuation calculated",{"$f":"B21*E21+B22*E22","v":0},"[dB]"]
[]
[]
["Notes:"]
["1) ... Summarize the length of all involved cables between transmitter and receiver."]
["2) ... Count the numbers of expanded Beam connections. The LC connection into transmitter and receiver has no effect."]
["        Example: Count 2 connections for one hybridMED cable and two hybridMED chassis. "]
[]
[]
[]
[]
["IMPORTANT !\nThis insertion loss calculator works with Excel macros, please select the macro security level \"medium\" or \"low\" when you want to work with it. Choose TOOLS / MACRO / SECURITY in the Excel pulldown menue to select the security level."]

{"sheet":"FIBERFOX","index":3,"n_rows":50,"n_cols":6,"rows_kept":50,"cut":false,"hidden":false,"merged":[[3,0,3,5],[49,0,53,5]]}
[]
[]
[]
["FIBERFOX Insertion Loss Calculator"]
[]
[]
["1. Mode and wavelength:"]
[]
[]
[]
[]
[]
["2. Attenuation properties:"]
[]
["Overal cable length 1)",0,"[m] (e.g. 150m)"]
["Number of cable connectors 2) ",0]
["Number of chassis connectors 3)",0]
[]
["3. Calculation:"]
[]
[null,null,null,"Typ.","Max."]
["     - Overal cable attenuation",{"$f":"B15/1000","v":0},"km of cable    x",0,0,"dB/km"]
["    - Overal cable connector attenuation",{"$f":"B16","v":0},"connector   ",0,0,"dB/con. "]
["    - Overal chassis connector attenuation",{"$f":"B17","v":0},"connector",0,0,"dB/con. "]
[" = Typical Link attenuation calculated",{"$f":"B22*D22+B23*D23+B24*D24","v":0},"[dB]"]
[" = Maximal Link attenuation calculated",{"$f":"B22*E22+B23*E23+B24*E24","v":0},"[dB]"]
[]
[]
["Notes:"]
["1) ... Summarize the length of all involved cables between transmitter and receiver."]
["2) ... Count the numbers of cable conntectors. One cable has two cable connectors."]
[]
[]
[]
[]
[]
[]
[]
[]
["3) ... Count the numbers of chassis connector. One cable needs two chassis connectors."]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["IMPORTANT !\nThis insertion loss calculator works with Excel macros, please select the macro security level \"medium\" or \"low\" when you want to work with it. Choose TOOLS / MACRO / SECURITY in the Excel pulldown menue to select the security level."]